**GENERAL PROPERTIES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **CONSTITUENT PROPERTIES** | **TEST METHOD** | **UNIT OF MEASURE** | **EN SPEC NUMBER** | **SPECIFICATION TOLERANCES** |
| **Material Thickness: 12 / 18mm** | Veneer callipers | mm |  | -0.5 / + 0.5 |
| **Average Dimensions:** |  |  |  |  |
| * **Length: 2000mm** | Tape measure | mm |  | -5 / + 5 |
| * **Width: 670mm** | Tape measure | mm |  | -5 / + 5 |
| * **Height: 15mm** | Veneer callipers | mm |  | -0.5 / + 0.5 |
| **Dimensional Tolerances:** |  |  |  |  |
| **Chemical Content (if any) – Define:** |  |  |  |  |
| **Residual Moisture Content:** |  |  |  |  |
| **Other – Please Specify:** |  |  |  |  |

**PRODUCT COMPOSITION [Please give the details for the largest capacity item in each range]**

**Country of Manufacture: ……………………………………………………………………………………**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ITEM** | **DIMENSIONAL THICKNESS** | **UNLADEN WEIGHT** | **TOTAL LOAD CAPACITY** | **STATIC LOAD TEST COMPLIANCE (Y/N)** | **ASH WEIGHT COMPLIANCE (Y/N)** |
| **Base:** | **30mm** |  |  |  |  |
| **Ends:** | **NA** |  |  |  |  |
| **Side:** | **NA** |  |  |  |  |
| **Lid:** | **NA** |  |  |  |  |
| **Total Product:** | **Av:** | **NA** | **NA** | **NA** | **NA** |

[NOTE: Unladen Weight and Total Load Capacity, Static Load and Ash Weight Compliance figures should be given for the total product and does not need to be recorded for each component]

**DESCRIPTION OF PRODUCTION/ASSEMBLY PROCESS**

|  |
| --- |
| Hand routered to shape using a template guided bit. |
| Holes for ties drilled |
| Edges sanded |
|  |
|  |